## AES

Device/Module Wishlist

Original topic on PlanetZ: https://forums.scopeusers.com/viewtopic.php?t=29621

#### AES

Posted: Tue Nov 16, 2010 8:59 am
by SART
Almost all contemporary DAW systems lets working at 96 and even 192 kHz (a.e. RME and others). It is VERY IMPORTANT also for XITE and for PCI cards (I mean a competition S-C with others). But it is possible only with S-C ADCs (A16) with Z-Link. Many S-C owners working with a preferable multichannel ADC - MYTEK, APOGEE, AURORA, LAVRY and others. Almost of them DO NOT HAVE A Z-LINK, but have multichannel AES or S/MUX outputs. An example APOGEE AD16 lets to write 16 channels at 96 Khz through AES or S/MUX interface.
Question: Why the S-C do not producing the Cards with optional AES-INs and S/MUX for 16-channel recordind?