## min/max hold in a device ?

Scope and XITE Development

Original topic on PlanetZ: https://forums.scopeusers.com/viewtopic.php?t=35123

#### min/max hold in a device ?

Posted: Sun Oct 08, 2017 11:25 am
by nebelfuerst
I want to make some module for measurement of some statistics.
Now I want to find the minimal and maximal BPM, which occured after reset.
Although this should be an easy job in C/C++, it doesn't seem so in the scope SDK.
I spotted the "if" and a "compare T" and compare W", and I have a BPM-value ready for display.
Who can I make a max-hold with that modules ?