## Ping-Pong Delay with midi sync

Device/Module Wishlist

Original topic on PlanetZ: https://forums.scopeusers.com/viewtopic.php?t=8597

####

Posted: Sat Feb 22, 2003 6:53 am
by aMo
If this already exists, show me.
All the CW delays sort of pan from left and not quite to the right, I want the delays to be panned to the extreeme left and the extreeme right (and no delay in the center)..
Might be possible to program the existing delays to to the job, but I would prefer a simple device with just pingpong..

####

Posted: Sun Mar 02, 2003 12:45 pm
by mr swim
I'm sure the Ztapper can do this.

####

Posted: Sun Mar 02, 2003 1:41 pm
by Michu
aMo
have you tried feeding signal just to left or just to right input of cw delay?

####

Posted: Sun Mar 02, 2003 1:57 pm
by aMo
Actually I found that the CW Multitap S delay could do the job, since I could turn the center delay off.
Thanx anyway
(Still want a Ping Pong delay though, would probably be less DSP-hungry than the multitap)

####

Posted: Sun Mar 02, 2003 7:54 pm
by ReD_MuZe
Hello amo? is there anyone in there?
read the post on top of you!
(DOH!)