## Soft Takeover For Controllers

Device/Module Wishlist

Original topic on PlanetZ: https://forums.scopeusers.com/viewtopic.php?t=8592

####

Posted: Fri Feb 21, 2003 3:49 pm
by huffcw
Want to move this to the wishlist since I found out it currently isn't implemented in SFP...
I am aware that the Creamware devices will respond appropriately to controllers with infinite dials. However, this is very limiting - as far as what controllers you can use with the system. I would rather not have to carry along more equipment (in addition to the keyboard I prefer to use as a controller).
SFP is suppose to be about ultimate flexibility, right. Therefore, I would like to see a soft takeover feature implemented in a future release of SFP. Many software synths have this - so why not SFP as well? It would benefit all users, because then you can use whatever controller you prefer without the problem of jumps.

####

Posted: Fri Feb 21, 2003 9:29 pm
by ReD_MuZe
im with you!!

####

Posted: Thu Feb 27, 2003 11:56 am
by huffcw
It would definitely help me out a lot and I sure a lot of other users (or at least make their setup much more effective if they don't have a controller with continuous dials).
I wonder if a third-party device might be able to make this work. Possibly a device that would go inbetween the midi input and the synth/mixer that would read the current location of the virtual knobs/slider than filter out incoming midi data until it goes past the point where the virtual knobs/sliders are at. Is it possible?

####

Posted: Thu Feb 27, 2003 1:57 pm
by at0m
Hi huffcw,
I replied in the Study Forum.
at0m.

####

Posted: Fri Feb 28, 2003 3:41 pm
by huffcw
Thanks for the reply - but how about setting this up in a virtual device for SFP that would convert any midi controller input to work this way?
The big thing here is being able to use any controller the user wants in SFP effectively. If there is a SFP device that could be placed between the midi input and the synth/mixer that would basically do the same thing as soft takeover or what you have described wtih the controller you use, that would be great.

####

Posted: Fri Mar 21, 2003 11:14 am
by huffcw
I found out the Event Electronics EZBus digital mixer/control surface has a special feature for the sliders that allows no jumps. It basically filters out the data of the sliders until they move past the point where the particular software knob/slider is at. If this feature could be developed into a SFP module, that would be great. Then, any hardware controller could be used the same way as the EZBus even if it doesn't have the special feature (as long as the SFP module is placed in front of the device being controlled).

####

Posted: Fri Mar 21, 2003 3:02 pm
by marcuspocus
I got the same feature in my home made midibox, it is called snap mode... The midi value will snap to fader once you pass over it, so no jump happen... Only thing i wish SFP could send 'snapshot' to update midi value for all controller...