## A new Scope/DP forum and 12-way signal switch?

Scope and XITE Development

Original topic on PlanetZ: https://forums.scopeusers.com/viewtopic.php?t=910

####

Posted: Mon Jun 18, 2001 11:46 am
by John Cooper
Hi Scope/DP folks,
Hope we'll have more success with this forum than we did with that ancient scope-dev@topica list
so, a question. i'm trying to make a 12-way signal switch.
i tried chaining up a couple 6 way switches, with a subtractor (-6) on the 2nd switch selector, and a mix on the two switch outputs. it works, but everytime it loads, i get "PepDisplayObject: IsPadRouted invalid value for the 1, argument Pad1". (click ok, and it all proceeds to work fine...)
anyone have a better solution (i.e. one that doesn't complain at load-time!)?
thanks
-john

####

Posted: Mon Jun 18, 2001 12:06 pm
by Obsidian
There's 1:4 and 4:1 switches in the Pulsar toolkit if you needed a specific switch coding up or wanted to use that one in cascade (for a commercial device) then mail me & we'll sort something out ;o)
BTW is this a public forum?

####

Posted: Mon Jun 18, 2001 12:28 pm
by John Cooper
it's a public forum, but for registered users only. in other words, no anonymous posting allowed, but otherwise it's open to the public.
scope/dp is a public product, right? so i don't see any reason reason to lock this down into a private forum. unless people can convince me otherwise!
-john

####

Posted: Mon Jun 18, 2001 1:01 pm
by huicholity
Hi,
and with the 'signal Switch EX' ? it seems possible to create a custom switch...
best regards,

####

Posted: Mon Jun 18, 2001 3:47 pm
by John Cooper
ha! i never noticed the 'signal Switch EX'.
thanks! that'll do nicely.
cheers,
-john