## Delay with Eq?

Device/Module Wishlist

Original topic on PlanetZ: https://forums.scopeusers.com/viewtopic.php?t=15561

####

Posted: Wed Mar 23, 2005 12:43 pm
by claudioD
Hello , does it exist a Deley plug-ing for Pulsar where it is possbile to set the EQ of the delay?
thx in advance

####

Posted: Wed Mar 23, 2005 1:53 pm
by wolf
yes, either the ChorusDelay from stw/warp69 or my MatrixDelay, where you can insert up to 3 effects (parallel or serial) in the feedback chain (beside others). I'm not shure about the echo from spacef .. but I'm shure it has something similar.
kind regards
Wolfgang

####

Posted: Wed Mar 23, 2005 2:37 pm
by samplaire
You can also have a look at Celmo's devices:
Tape Echo Sim
Celmo Echo Q
EchoreQ 2
Ganja Dub Delay
Pro Series Vintage Delay Line

####

Posted: Wed Mar 23, 2005 2:57 pm
by at0m
Or cook one at home

####

Posted: Wed Mar 23, 2005 3:37 pm
by spacef
hi, wolf, thanks for mentionning.
of course (!) in Echo you can "also" insert an eq if you wish in stereo (pre-delay, or in-fb-loop, or post delay). you can use the satellite insert slot and use one of the satellite filters which also include several eqs (Air/Aerial or Mega Eq) or any of the other satellites/RD filters, and select the routing of those satellites (ie, pre or post delay, and/or chained with the included LP/HP/BP/Voxal (formant style) filters, and use one of the modulation source to modulate those staellite filters/eqs
I have a freeware delay where you can isert an eq if you wish (if i remember well )
just visit http://www.spacef.com "freeware" page of the forum (see menu at the left). i haven't been there lately, so im not sure which delay it is (i think it is the very simple "tempo delay 1", which has nothing to do with Echo, but probably allows to do what you wish).
best regards.
Mehdi

####

Posted: Wed Mar 23, 2005 3:38 pm
by samplaire
@at0m|c:
Input, more input!
{Isn't this one for Mod3 only? I tried to launch it and a registration dialog box appeared for modular}

####

Posted: Wed Mar 23, 2005 4:16 pm
by at0m
It's suddenly become mod2 :>
ConstB sets Dry/Wet balance, and set feedback level on lower insert volume knobs for example.